SECTION 11 6833

**PART 1 GENERAL**

* 1. RELATED WORK

Review Contract Documents for requirements that affect work of this section. Specification sections that directly relate to work of this section include, but are not limited to:

        Section 33 3000 – Site Improvements

Section 32 1826 - Synthetic Grass Surfacing

        Section 32 1822 – Synthetic Athletic & Sports Surfacing

        Section 12 9300 – Site Furnishings

        Section 03 3000 – Cast-in-Place Concrete

Section 11 6500 – Athletic & Recreational Equipment

1.02 SUBMITTALS

A. Product Data: Submit manufacturer’s product literature, technical specifications, and other data required to demonstrate compliance with specified requirements for all athletic equipment.

1.03 QUALITY ASSURANCE

A. Fabrication and installation of site improvements by experienced craftsmen with excellent record of performance on completed projects of comparable size, scope, and quality.

 B. All materials, hardware and furnishings shall be new, first quality.

1.04 FIELD MEASUREMENTS

A. Contractor shall verify position and layout of all athletic field equipment. Verify dimensions by field measurements.

* 1. SYSTEM DESCRIPTION

A. 20’ Baseball Foul Pole **#SEBBFP-20.**

**PART 2 - PRODUCTS**

2.01 MANUFACTURERS/SUPPLIERS

A. Manufacturers/Suppliers and product selections named are provided to establish the minimum standard and shall comply with the following by:

SportsEdge®

P.O. Box 837

259 Murdock Rd.

Troutman, NC 28166

PH: 800-334-6057

FX: 704-528-0179

info@sportsedge.com

www.sportsedge.com

2.02 BASEBALL / SOFTBALL PRODUCTS

 A. General: Provide equipment complying with the following requirements.

B. FOUL POLES: 20’ Baseball Foul Pole, Model **SEBBF-20** shall be manufactured to meet the following criteria as the minimum standard:

1. Main Upright: Fabricated of 3.5” O.D. heavy wall steel pipe, 24’ long (20’2” above ground). *Designer select:* Direct embedment or inserted into embedded sleeve.

2. Cap: Domed fence cap installed to top of pole.

3. Wing Panel: Two sections of heavy-duty 18” x 60” x 2” – 11-gauge, steel sheet metal panel. Panels are bolted to pole section and are secured to each other at their outer edges.

4. Finish: The entire baseball foul pole assembly shall be finished in a durable yellow powder-coated finish over zinc rich primer.

5. OPTIONAL: Ground Sleeve: Steel, model **#FPS-20**

**PART 3: EXECUTION**

3.03 INSTALLATION

A. All athletic equipment shall be installed as recommended by manufacturer's

 written directions, and as indicated on the drawings.

 END OF SECTION